 -- Copyright (C) 1991-2012 Altera Corporation
 -- Your use of Altera Corporation's design tools, logic functions 
 -- and other software and tools, and its AMPP partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Altera Program License 
 -- Subscription Agreement, Altera MegaCore Function License 
 -- Agreement, or other applicable license agreement, including, 
 -- without limitation, that your use is for the sole purpose of 
 -- programming logic devices manufactured by Altera and sold by 
 -- Altera or its authorized distributors.  Please refer to the 
 -- applicable agreement for further details.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCCPGM        : Dedicated power pin for configuration, which MUST be connected to 1.8V, 2.5V or 3.0V depending on the requirements of the configuration device.
 -- VCCINT        : Dedicated power pin, which MUST be connected to VCC  (1.2V).
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 --					Bank 3:		3.3V
 --					Bank 4:		2.5V
 --					Bank 5:		2.5V
 --					Bank 6:		3.3V
 --					Bank 7:		1.8V
 --					Bank 8:		1.8V
 --					Bank 9:	3.3V
 -- RREF          : External reference resistor for the quad, MUST be connected to
 --                 GND via a 2k Ohm resistor.
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin.   For transceiver I/O banks, connect each pin marked GND*
 --           	    either individually through a 10k Ohm resistor to GND or tie all pins
 --           	    together and connect through a single 10k Ohm resistor to GND.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 -- GXB_GND*      : Unused GXB Receiver or dedicated reference clock pin. This pin
 --                 must be connected to GXB_GND through a 10k Ohm resistor.
 -- GXB_NC        : Unused GXB Transmitter or dedicated clock output pin. This pin
 --                 must not be connected.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus II 32-bit Version 12.0 Build 263 08/02/2012 Service Pack 2 SJ Full Version
CHIP  "golden_top"  ASSIGNED TO AN: EP4CGX22CF19C8

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
GND                          : A1        : gnd    :                   :         :           :                
GND                          : A2        : gnd    :                   :         :           :                
GND                          : A3        : gnd    :                   :         :           :                
epcs_flash_controller_data0  : A4        : input  : 3.3-V LVTTL       :         : 9         : Y              
ddr2_memory_mem_cs_n         : A5        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[15]       : A6        : bidir  : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[8]        : A7        : bidir  : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[9]        : A8        : bidir  : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_ba[1]        : A9        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[10]       : A10       : bidir  : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[13]       : A11       : bidir  : SSTL-18 Class I   :         : 8         : Y              
GND+                         : A12       :        :                   :         : 7         :                
ddr2_memory_mem_dq[3]        : A13       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[2]      : A14       : output : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[7]      : A15       : output : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[11]     : A16       : output : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_dq[5]        : A17       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[4]      : A18       : output : SSTL-18 Class I   :         : 7         : Y              
GXB_NC                       : B1        :        :                   :         : QL0       :                
GXB_NC                       : B2        :        :                   :         : QL0       :                
GND                          : B3        : gnd    :                   :         :           :                
epcs_flash_controller_sdo    : B4        : output : 3.3-V LVTTL       :         : 9         : Y              
ddr2_memory_mem_odt          : B5        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dm[1]        : B6        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[14]       : B7        : bidir  : SSTL-18 Class I   :         : 8         : Y              
GND                          : B8        : gnd    :                   :         :           :                
ddr2_memory_mem_ba[0]        : B9        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[11]       : B10       : bidir  : SSTL-18 Class I   :         : 8         : Y              
GND                          : B11       : gnd    :                   :         :           :                
GND+                         : B12       :        :                   :         : 7         :                
ddr2_memory_mem_addr[5]      : B13       : output : SSTL-18 Class I   :         : 7         : Y              
GND                          : B14       : gnd    :                   :         :           :                
ddr2_memory_mem_dq[7]        : B15       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[6]      : B16       : output : SSTL-18 Class I   :         : 7         : Y              
GND                          : B17       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : B18       :        :                   :         : 7         :                
GND                          : C1        : gnd    :                   :         :           :                
GND                          : C2        : gnd    :                   :         :           :                
GND                          : C3        : gnd    :                   :         :           :                
nCONFIG                      : C4        :        :                   :         : 9         :                
epcs_flash_controller_sce    : C5        : output : 3.3-V LVTTL       :         : 9         : Y              
ddr2_memory_mem_cas_n        : C6        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_we_n         : C7        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dqs[1]       : C8        : bidir  : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_addr[0]      : C9        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[12]       : C10       : bidir  : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_addr[10]     : C11       : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[1]        : C12       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[12]     : C13       : output : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_dqs[0]       : C14       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_dq[0]        : C15       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_clk_n        : C16       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_clk          : C17       : bidir  : SSTL-18 Class I   :         : 7         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : C18       :        :                   :         : 7         :                
GXB_GND*                     : D1        :        :                   :         : QL0       :                
GXB_GND*                     : D2        :        :                   :         : QL0       :                
nCE                          : D3        :        :                   :         : 9         :                
TDI                          : D4        : input  :                   :         : 9         :                
epcs_flash_controller_dclk   : D5        : output : 3.3-V LVTTL       :         : 9         : Y              
ddr2_memory_mem_ras_n        : D6        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_cke          : D7        : output : SSTL-18 Class I   :         : 8         : Y              
VREFB8N0                     : D8        :        :                   : 0.9V    : 8         :                
ddr2_memory_mem_ba[2]        : D9        : output : SSTL-18 Class I   :         : 8         : Y              
ddr2_memory_mem_dq[6]        : D10       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_dq[4]        : D11       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[1]      : D12       : output : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[3]      : D13       : output : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[9]      : D14       : output : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_dq[2]        : D15       : bidir  : SSTL-18 Class I   :         : 7         : Y              
ddr2_memory_mem_addr[8]      : D16       : output : SSTL-18 Class I   :         : 7         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : D17       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D18       :        :                   :         : 6         :                
GND                          : E1        : gnd    :                   :         :           :                
GND                          : E2        : gnd    :                   :         :           :                
TMS                          : E3        : input  :                   :         : 9         :                
TDO                          : E4        : output :                   :         : 9         :                
TCK                          : E5        : input  :                   :         : 9         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : E6        :        :                   :         : 8         :                
VCCIO8                       : E7        : power  :                   : 1.8V    : 8         :                
GND                          : E8        : gnd    :                   :         :           :                
VCCIO8                       : E9        : power  :                   : 1.8V    : 8         :                
ddr2_memory_mem_dm[0]        : E10       : output : SSTL-18 Class I   :         : 7         : Y              
GND                          : E11       : gnd    :                   :         :           :                
VREFB7N0                     : E12       :        :                   : 0.9V    : 7         :                
VCCIO7                       : E13       : power  :                   : 1.8V    : 7         :                
GND                          : E14       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : E15       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : E16       :        :                   :         : 6         :                
GND                          : E17       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : E18       :        :                   :         : 6         :                
GXB_NC                       : F1        :        :                   :         : QL0       :                
GXB_NC                       : F2        :        :                   :         : QL0       :                
VCCL_GXB                     : F3        : power  :                   : 1.2V    :           :                
VCCIO9                       : F4        : power  :                   : 3.3V    : 9         :                
GND                          : F5        : gnd    :                   :         :           :                
VCCD_PLL                     : F6        : power  :                   : 1.2V    :           :                
VCCINT                       : F7        : power  :                   : 1.2V    :           :                
VCCIO8                       : F8        : power  :                   : 1.8V    : 8         :                
VCC_CLKIN8A                  : F9        : power  :                   : 2.5V    : 8A        :                
VCCIO7                       : F10       : power  :                   : 1.8V    : 7         :                
VCCIO7                       : F11       : power  :                   : 1.8V    : 7         :                
VCCIO7                       : F12       : power  :                   : 1.8V    : 7         :                
GND                          : F13       : gnd    :                   :         :           :                
VCCD_PLL                     : F14       : power  :                   : 1.2V    :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : F15       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : F16       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : F17       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : F18       :        :                   :         : 6         :                
GND                          : G1        : gnd    :                   :         :           :                
GND                          : G2        : gnd    :                   :         :           :                
VCCH_GXB                     : G3        : power  :                   : 2.5V    :           :                
VCCINT                       : G4        : power  :                   : 1.2V    :           :                
VCCA                         : G5        : power  :                   : 2.5V    :           :                
VCCINT                       : G6        : power  :                   : 1.2V    :           :                
GND                          : G7        : gnd    :                   :         :           :                
VCCINT                       : G8        : power  :                   : 1.2V    :           :                
clk_125M(n)                  : G9        : input  : LVDS              :         : 8A        : Y              
clk_125M                     : G10       : input  : LVDS              :         : 8A        : Y              
GND                          : G11       : gnd    :                   :         :           :                
VCCINT                       : G12       : power  :                   : 1.2V    :           :                
VCCA                         : G13       : power  :                   : 2.5V    :           :                
VCCIO6                       : G14       : power  :                   : 3.3V    : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G15       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G16       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G17       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G18       :        :                   :         : 6         :                
GXB_GND*                     : H1        :        :                   :         : QL0       :                
GXB_GND*                     : H2        :        :                   :         : QL0       :                
VCCL_GXB                     : H3        : power  :                   : 1.2V    :           :                
GND                          : H4        : gnd    :                   :         :           :                
VCCINT                       : H5        : power  :                   : 1.2V    :           :                
GND                          : H6        : gnd    :                   :         :           :                
VCCINT                       : H7        : power  :                   : 1.2V    :           :                
GND                          : H8        : gnd    :                   :         :           :                
VCCINT                       : H9        : power  :                   : 1.2V    :           :                
GND                          : H10       : gnd    :                   :         :           :                
VCCINT                       : H11       : power  :                   : 1.2V    :           :                
GND                          : H12       : gnd    :                   :         :           :                
VCCINT                       : H13       : power  :                   : 1.2V    :           :                
GND                          : H14       : gnd    :                   :         :           :                
VCCIO6                       : H15       : power  :                   : 3.3V    : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : H16       :        :                   :         : 6         :                
GND                          : H17       : gnd    :                   :         :           :                
GND+                         : H18       :        :                   :         : 6         :                
GND                          : J1        : gnd    :                   :         :           :                
GND                          : J2        : gnd    :                   :         :           :                
VCCA_GXB                     : J3        : power  :                   : 2.5V    :           :                
VCCINT                       : J4        : power  :                   : 1.2V    :           :                
GND                          : J5        : gnd    :                   :         :           :                
VCCINT                       : J6        : power  :                   : 1.2V    :           :                
GND                          : J7        : gnd    :                   :         :           :                
VCCINT                       : J8        : power  :                   : 1.2V    :           :                
GND                          : J9        : gnd    :                   :         :           :                
VCCINT                       : J10       : power  :                   : 1.2V    :           :                
GND                          : J11       : gnd    :                   :         :           :                
VCCINT                       : J12       : power  :                   : 1.2V    :           :                
GND                          : J13       : gnd    :                   :         :           :                
VCCINT                       : J14       : power  :                   : 1.2V    :           :                
VCCIO6                       : J15       : power  :                   : 3.3V    : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J16       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J17       :        :                   :         : 6         :                
ext_reset_n                  : J18       : input  : 3.3-V LVTTL       :         : 6         : Y              
GXB_NC                       : K1        :        :                   :         : QL0       :                
GXB_NC                       : K2        :        :                   :         : QL0       :                
VCCL_GXB                     : K3        : power  :                   : 1.2V    :           :                
GND                          : K4        : gnd    :                   :         :           :                
VCCINT                       : K5        : power  :                   : 1.2V    :           :                
GND                          : K6        : gnd    :                   :         :           :                
VCCINT                       : K7        : power  :                   : 1.2V    :           :                
GND                          : K8        : gnd    :                   :         :           :                
VCCINT                       : K9        : power  :                   : 1.2V    :           :                
GND                          : K10       : gnd    :                   :         :           :                
VCCINT                       : K11       : power  :                   : 1.2V    :           :                
GND                          : K12       : gnd    :                   :         :           :                
VCCINT                       : K13       : power  :                   : 1.2V    :           :                
VCCIO5                       : K14       : power  :                   : 2.5V    : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : K15       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : K16       :        :                   :         : 5         :                
tse_mac_rx_clk               : K17       : input  : 2.5 V             :         : 5         : Y              
GND+                         : K18       :        :                   :         : 5         :                
GND                          : L1        : gnd    :                   :         :           :                
GND                          : L2        : gnd    :                   :         :           :                
VCCH_GXB                     : L3        : power  :                   : 2.5V    :           :                
VCCINT                       : L4        : power  :                   : 1.2V    :           :                
GND                          : L5        : gnd    :                   :         :           :                
VCCA                         : L6        : power  :                   : 2.5V    :           :                
GND                          : L7        : gnd    :                   :         :           :                
VCCINT                       : L8        : power  :                   : 1.2V    :           :                
GND                          : L9        : gnd    :                   :         :           :                
VCCINT                       : L10       : power  :                   : 1.2V    :           :                
GND                          : L11       : gnd    :                   :         :           :                
VCCINT                       : L12       : power  :                   : 1.2V    :           :                
VCCA                         : L13       : power  :                   : 2.5V    :           :                
GND                          : L14       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L15       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L16       :        :                   :         : 5         :                
GND                          : L17       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L18       :        :                   :         : 5         :                
GXB_GND*                     : M1        :        :                   :         : QL0       :                
GXB_GND*                     : M2        :        :                   :         : QL0       :                
VCCL_GXB                     : M3        : power  :                   : 1.2V    :           :                
GND                          : M4        : gnd    :                   :         :           :                
VCCD_PLL                     : M5        : power  :                   : 1.2V    :           :                
GND                          : M6        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M7        :        :                   :         : 3         :                
GND                          : M8        : gnd    :                   :         :           :                
clk_100M                     : M9        : input  : LVDS              :         : 3A        : Y              
clk_100M(n)                  : M10       : input  : LVDS              :         : 3A        : Y              
VCCINT                       : M11       : power  :                   : 1.2V    :           :                
GND                          : M12       : gnd    :                   :         :           :                
GND                          : M13       : gnd    :                   :         :           :                
VCCD_PLL                     : M14       : power  :                   : 1.2V    :           :                
VCCIO5                       : M15       : power  :                   : 2.5V    : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M16       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M17       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M18       :        :                   :         : 5         :                
GND                          : N1        : gnd    :                   :         :           :                
GND                          : N2        : gnd    :                   :         :           :                
VCCA_GXB                     : N3        : power  :                   : 2.5V    :           :                
VCCINT                       : N4        : power  :                   : 1.2V    :           :                
sd_card_clk                  : N5        : output : 3.3-V LVTTL       :         : 3         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : N6        :        :                   :         : 3         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N7        :        :                   :         : 3         :                
VCCIO3                       : N8        : power  :                   : 3.3V    : 3         :                
VCC_CLKIN3A                  : N9        : power  :                   : 2.5V    : 3A        :                
GND                          : N10       : gnd    :                   :         :           :                
VCCIO4                       : N11       : power  :                   : 2.5V    : 4         :                
VCCIO4                       : N12       : power  :                   : 2.5V    : 4         :                
VCCIO4                       : N13       : power  :                   : 2.5V    : 4         :                
VCCIO4                       : N14       : power  :                   : 2.5V    : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N15       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N16       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N17       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N18       :        :                   :         : 5         :                
GXB_NC                       : P1        :        :                   :         : QL0       :                
GXB_NC                       : P2        :        :                   :         : QL0       :                
GND                          : P3        : gnd    :                   :         :           :                
MSEL2                        : P4        :        :                   :         : 3         :                
GND                          : P5        : gnd    :                   :         :           :                
alive_led                    : P6        : output : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : P7        : power  :                   : 3.3V    : 3         :                
GND                          : P8        : gnd    :                   :         :           :                
VCCIO3                       : P9        : power  :                   : 3.3V    : 3         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : P10       :        :                   :         : 3         :                
GND                          : P11       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : P12       :        :                   :         : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : P13       :        :                   :         : 4         :                
GND                          : P14       : gnd    :                   :         :           :                
tse_mac_gtx_clk              : P15       : output : 2.5 V             :         : 4         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : P16       :        :                   :         : 5         :                
GND                          : P17       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : P18       :        :                   :         : 5         :                
GND                          : R1        : gnd    :                   :         :           :                
GND                          : R2        : gnd    :                   :         :           :                
GND                          : R3        : gnd    :                   :         :           :                
VCCL_GXB                     : R4        : power  :                   : 1.2V    :           :                
MSEL1                        : R5        :        :                   :         : 3         :                
~ALTERA_NCEO~ / RESERVED_OUTPUT_OPEN_DRAIN : R6        : output : 3.3-V LVTTL       :         : 3         : N              
RESERVED_INPUT_WITH_WEAK_PULLUP : R7        :        :                   :         : 3         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R8        :        :                   :         : 3         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R9        :        :                   :         : 3         :                
led[3]                       : R10       : output : 3.3-V LVTTL       :         : 3         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : R11       :        :                   :         : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R12       :        :                   :         : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R13       :        :                   :         : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R14       :        :                   :         : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R15       :        :                   :         : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R16       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R17       :        :                   :         : 5         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R18       :        :                   :         : 5         :                
GXB_GND*                     : T1        :        :                   :         : QL0       :                
GXB_GND*                     : T2        :        :                   :         : QL0       :                
GND                          : T3        : gnd    :                   :         :           :                
VCCA_GXB                     : T4        : power  :                   : 2.5V    :           :                
MSEL0                        : T5        :        :                   :         : 3         :                
button_pio                   : T6        : input  : 3.3-V LVTTL       :         : 3         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : T7        :        :                   :         : 3         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : T8        :        :                   :         : 3         :                
sd_card_cs_n                 : T9        : output : 3.3-V LVTTL       :         : 3         : Y              
led[0]                       : T10       : output : 3.3-V LVTTL       :         : 3         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : T11       :        :                   :         : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : T12       :        :                   :         : 4         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : T13       :        :                   :         : 4         :                
tse_mac_rx_control           : T14       : input  : 2.5 V             :         : 4         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : T15       :        :                   :         : 4         :                
tse_mac_rgmii_out[1]         : T16       : output : 2.5 V             :         : 4         : Y              
tse_mac_rgmii_out[0]         : T17       : output : 2.5 V             :         : 4         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : T18       :        :                   :         : 5         :                
GND                          : U1        : gnd    :                   :         :           :                
GND                          : U2        : gnd    :                   :         :           :                
NC                           : U3        :        :                   :         :           :                
CONF_DONE                    : U4        :        :                   :         : 3         :                
GND                          : U5        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : U6        :        :                   :         : 3         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : U7        :        :                   :         : 3         :                
GND                          : U8        : gnd    :                   :         :           :                
sd_card_data_out             : U9        : output : 3.3-V LVTTL       :         : 3         : Y              
led[2]                       : U10       : output : 3.3-V LVTTL       :         : 3         : Y              
GND                          : U11       : gnd    :                   :         :           :                
tse_mac_mdio                 : U12       : bidir  : 2.5 V             :         : 4         : Y              
tse_mac_resetn               : U13       : output : 2.5 V             :         : 4         : Y              
GND                          : U14       : gnd    :                   :         :           :                
tse_mac_rgmii_in[2]          : U15       : input  : 2.5 V             :         : 4         : Y              
tse_mac_tx_control           : U16       : output : 2.5 V             :         : 4         : Y              
GND                          : U17       : gnd    :                   :         :           :                
tse_mac_rgmii_out[2]         : U18       : output : 2.5 V             :         : 4         : Y              
RREF                         : V1        :        :                   :         :           :                
GND                          : V2        : gnd    :                   :         :           :                
NC                           : V3        :        :                   :         :           :                
nSTATUS                      : V4        :        :                   :         : 3         :                
L0_led                       : V5        : output : 3.3-V LVTTL       :         : 3         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : V6        :        :                   :         : 3         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : V7        :        :                   :         : 3         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : V8        :        :                   :         : 3         :                
sd_card_data_in              : V9        : input  : 3.3-V LVTTL       :         : 3         : Y              
led[1]                       : V10       : output : 3.3-V LVTTL       :         : 3         : Y              
pcie_rst_n                   : V11       : input  : 2.5 V             :         : 4         : Y              
clk_50M                      : V12       : input  : 2.5 V             :         : 4         : Y              
tse_mac_mdc                  : V13       : output : 2.5 V             :         : 4         : Y              
tse_mac_rgmii_in[0]          : V14       : input  : 2.5 V             :         : 4         : Y              
tse_mac_rgmii_in[1]          : V15       : input  : 2.5 V             :         : 4         : Y              
tse_mac_rgmii_in[3]          : V16       : input  : 2.5 V             :         : 4         : Y              
tse_mac_rgmii_out[3]         : V17       : output : 2.5 V             :         : 4         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : V18       :        :                   :         : 4         :                
