/*
 * linker.x - Linker script
 *
 * Machine generated for CPU 'CPU' in SOPC Builder design 'FULL_SYS'
 * SOPC Builder design path: D:/Work_Dir/Demos/cytech_kit/Easy_GX/Examples/NIOS_demo/FULL_SYS.sopcinfo
 *
 * Generated: Mon Sep 03 10:52:54 CST 2012
 */

/*
 * DO NOT MODIFY THIS FILE
 *
 * Changing this file will have subtle consequences
 * which will almost certainly lead to a nonfunctioning
 * system. If you do modify this file, be aware that your
 * changes will be overwritten and lost when this file
 * is generated again.
 *
 * DO NOT MODIFY THIS FILE
 */

/*
 * License Agreement
 *
 * Copyright (c) 2008
 * Altera Corporation, San Jose, California, USA.
 * All rights reserved.
 *
 * Permission is hereby granted, free of charge, to any person obtaining a
 * copy of this software and associated documentation files (the "Software"),
 * to deal in the Software without restriction, including without limitation
 * the rights to use, copy, modify, merge, publish, distribute, sublicense,
 * and/or sell copies of the Software, and to permit persons to whom the
 * Software is furnished to do so, subject to the following conditions:
 *
 * The above copyright notice and this permission notice shall be included in
 * all copies or substantial portions of the Software.
 *
 * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
 * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
 * FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
 * AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
 * LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 * FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER
 * DEALINGS IN THE SOFTWARE.
 *
 * This agreement shall be governed in all respects by the laws of the State
 * of California and by the laws of the United States of America.
 */

MEMORY
{
    reset : ORIGIN = 0x0, LENGTH = 32
    epcs_flash_controller : ORIGIN = 0x20, LENGTH = 2016
    descriptor_memory : ORIGIN = 0x1000, LENGTH = 4096
    RAM_BEFORE_EXCEPTION : ORIGIN = 0x8000, LENGTH = 32
    RAM : ORIGIN = 0x8020, LENGTH = 4064
    ext_flash : ORIGIN = 0x2000000, LENGTH = 16777216
    DDR2 : ORIGIN = 0x8000000, LENGTH = 67108864
}

/* Define symbols for each memory base-address */
__alt_mem_epcs_flash_controller = 0x0;
__alt_mem_descriptor_memory = 0x1000;
__alt_mem_RAM = 0x8000;
__alt_mem_ext_flash = 0x2000000;
__alt_mem_DDR2 = 0x8000000;

OUTPUT_FORMAT( "elf32-littlenios2",
               "elf32-littlenios2",
               "elf32-littlenios2" )
OUTPUT_ARCH( nios2 )
ENTRY( _start )

/*
 * The alt_load() facility is disabled. This typically happens when an
 * external bootloader is provided or the application runs in place.
 * The LMA (aka physical address) of each section defaults to its VMA.
 */

SECTIONS
{

    /*
     * Output sections associated with reset and exceptions (they have to be first)
     */

    .entry :
    {
        KEEP (*(.entry))
    } > reset

    .exceptions :
    {
        PROVIDE (__ram_exceptions_start = ABSOLUTE(.));
        . = ALIGN(0x20);
        KEEP (*(.irq));
        KEEP (*(.exceptions.entry.label));
        KEEP (*(.exceptions.entry.user));
        KEEP (*(.exceptions.entry));
        KEEP (*(.exceptions.irqtest.user));
        KEEP (*(.exceptions.irqtest));
        KEEP (*(.exceptions.irqhandler.user));
        KEEP (*(.exceptions.irqhandler));
        KEEP (*(.exceptions.irqreturn.user));
        KEEP (*(.exceptions.irqreturn));
        KEEP (*(.exceptions.notirq.label));
        KEEP (*(.exceptions.notirq.user));
        KEEP (*(.exceptions.notirq));
        KEEP (*(.exceptions.soft.user));
        KEEP (*(.exceptions.soft));
        KEEP (*(.exceptions.unknown.user));
        KEEP (*(.exceptions.unknown));
        KEEP (*(.exceptions.exit.label));
        KEEP (*(.exceptions.exit.user));
        KEEP (*(.exceptions.exit));
        KEEP (*(.exceptions));
        PROVIDE (__ram_exceptions_end = ABSOLUTE(.));
    } > RAM

    PROVIDE (__flash_exceptions_start = LOADADDR(.exceptions));

    .text :
    {
        /*
         * All code sections are merged into the text output section, along with
         * the read only data sections.
         *
         */

        PROVIDE (stext = ABSOLUTE(.));

        *(.interp)
        *(.hash)
        *(.dynsym)
        *(.dynstr)
        *(.gnu.version)
        *(.gnu.version_d)
        *(.gnu.version_r)
        *(.rel.init)
        *(.rela.init)
        *(.rel.text .rel.text.* .rel.gnu.linkonce.t.*)
        *(.rela.text .rela.text.* .rela.gnu.linkonce.t.*)
        *(.rel.fini)
        *(.rela.fini)
        *(.rel.rodata .rel.rodata.* .rel.gnu.linkonce.r.*)
        *(.rela.rodata .rela.rodata.* .rela.gnu.linkonce.r.*)
        *(.rel.data .rel.data.* .rel.gnu.linkonce.d.*)
        *(.rela.data .rela.data.* .rela.gnu.linkonce.d.*)
        *(.rel.tdata .rel.tdata.* .rel.gnu.linkonce.td.*)
        *(.rela.tdata .rela.tdata.* .rela.gnu.linkonce.td.*)
        *(.rel.tbss .rel.tbss.* .rel.gnu.linkonce.tb.*)
        *(.rela.tbss .rela.tbss.* .rela.gnu.linkonce.tb.*)
        *(.rel.ctors)
        *(.rela.ctors)
        *(.rel.dtors)
        *(.rela.dtors)
        *(.rel.got)
        *(.rela.got)
        *(.rel.sdata .rel.sdata.* .rel.gnu.linkonce.s.*)
        *(.rela.sdata .rela.sdata.* .rela.gnu.linkonce.s.*)
        *(.rel.sbss .rel.sbss.* .rel.gnu.linkonce.sb.*)
        *(.rela.sbss .rela.sbss.* .rela.gnu.linkonce.sb.*)
        *(.rel.sdata2 .rel.sdata2.* .rel.gnu.linkonce.s2.*)
        *(.rela.sdata2 .rela.sdata2.* .rela.gnu.linkonce.s2.*)
        *(.rel.sbss2 .rel.sbss2.* .rel.gnu.linkonce.sb2.*)
        *(.rela.sbss2 .rela.sbss2.* .rela.gnu.linkonce.sb2.*)
        *(.rel.bss .rel.bss.* .rel.gnu.linkonce.b.*)
        *(.rela.bss .rela.bss.* .rela.gnu.linkonce.b.*)
        *(.rel.plt)
        *(.rela.plt)
        *(.rel.dyn)

        KEEP (*(.init))
        *(.plt)
        *(.text .stub .text.* .gnu.linkonce.t.*)

        /* .gnu.warning sections are handled specially by elf32.em.  */

        *(.gnu.warning.*)
        KEEP (*(.fini))
        PROVIDE (__etext = ABSOLUTE(.));
        PROVIDE (_etext = ABSOLUTE(.));
        PROVIDE (etext = ABSOLUTE(.));

        *(.eh_frame_hdr)
        /* Ensure the __preinit_array_start label is properly aligned.  We
           could instead move the label definition inside the section, but
           the linker would then create the section even if it turns out to
           be empty, which isn't pretty.  */
        . = ALIGN(4);
        PROVIDE (__preinit_array_start = ABSOLUTE(.));
        *(.preinit_array)
        PROVIDE (__preinit_array_end = ABSOLUTE(.));
        PROVIDE (__init_array_start = ABSOLUTE(.));
        *(.init_array)
        PROVIDE (__init_array_end = ABSOLUTE(.));
        PROVIDE (__fini_array_start = ABSOLUTE(.));
        *(.fini_array)
        PROVIDE (__fini_array_end = ABSOLUTE(.));
        SORT(CONSTRUCTORS)
        KEEP (*(.eh_frame))
        *(.gcc_except_table)
        *(.dynamic)
        PROVIDE (__CTOR_LIST__ = ABSOLUTE(.));
        KEEP (*(.ctors))
        KEEP (*(SORT(.ctors.*)))
        PROVIDE (__CTOR_END__ = ABSOLUTE(.));
        PROVIDE (__DTOR_LIST__ = ABSOLUTE(.));
        KEEP (*(.dtors))
        KEEP (*(SORT(.dtors.*)))
        PROVIDE (__DTOR_END__ = ABSOLUTE(.));
        KEEP (*(.jcr))
        . = ALIGN(4);
    } > DDR2 = 0x3a880100 /* Nios II NOP instruction */

    .rodata :
    {
        PROVIDE (__ram_rodata_start = ABSOLUTE(.));
        . = ALIGN(4);
        *(.rodata .rodata.* .gnu.linkonce.r.*)
        *(.rodata1)
        . = ALIGN(4);
        PROVIDE (__ram_rodata_end = ABSOLUTE(.));
    } > DDR2

    PROVIDE (__flash_rodata_start = LOADADDR(.rodata));

    .rwdata :
    {
        PROVIDE (__ram_rwdata_start = ABSOLUTE(.));
        . = ALIGN(4);
        *(.got.plt) *(.got)
        *(.data1)
        *(.data .data.* .gnu.linkonce.d.*)

        _gp = ABSOLUTE(. + 0x8000);
        PROVIDE(gp = _gp);

        *(.rwdata .rwdata.*)
        *(.sdata .sdata.* .gnu.linkonce.s.*)
        *(.sdata2 .sdata2.* .gnu.linkonce.s2.*)

        . = ALIGN(4);
        _edata = ABSOLUTE(.);
        PROVIDE (edata = ABSOLUTE(.));
        PROVIDE (__ram_rwdata_end = ABSOLUTE(.));
    } > DDR2

    PROVIDE (__flash_rwdata_start = LOADADDR(.rwdata));

    .bss :
    {
        __bss_start = ABSOLUTE(.);
        PROVIDE (__sbss_start = ABSOLUTE(.));
        PROVIDE (___sbss_start = ABSOLUTE(.));

        *(.dynsbss)
        *(.sbss .sbss.* .gnu.linkonce.sb.*)
        *(.sbss2 .sbss2.* .gnu.linkonce.sb2.*)
        *(.scommon)

        PROVIDE (__sbss_end = ABSOLUTE(.));
        PROVIDE (___sbss_end = ABSOLUTE(.));

        *(.dynbss)
        *(.bss .bss.* .gnu.linkonce.b.*)
        *(COMMON)

        . = ALIGN(4);
        __bss_end = ABSOLUTE(.);
    } > DDR2

    /*
     *
     * One output section mapped to the associated memory device for each of
     * the available memory devices. These are not used by default, but can
     * be used by user applications by using the .section directive.
     *
     * The output section used for the heap is treated in a special way,
     * i.e. the symbols "end" and "_end" are added to point to the heap start.
     *
     */

    .epcs_flash_controller :
    {
        PROVIDE (_alt_partition_epcs_flash_controller_start = ABSOLUTE(.));
        *(.epcs_flash_controller. epcs_flash_controller.*)
        . = ALIGN(4);
        PROVIDE (_alt_partition_epcs_flash_controller_end = ABSOLUTE(.));
    } > epcs_flash_controller

    PROVIDE (_alt_partition_epcs_flash_controller_load_addr = LOADADDR(.epcs_flash_controller));

    .descriptor_memory :
    {
        PROVIDE (_alt_partition_descriptor_memory_start = ABSOLUTE(.));
        *(.descriptor_memory. descriptor_memory.*)
        . = ALIGN(4);
        PROVIDE (_alt_partition_descriptor_memory_end = ABSOLUTE(.));
    } > descriptor_memory

    PROVIDE (_alt_partition_descriptor_memory_load_addr = LOADADDR(.descriptor_memory));

    .RAM :
    {
        PROVIDE (_alt_partition_RAM_start = ABSOLUTE(.));
        *(.RAM. RAM.*)
        . = ALIGN(4);
        PROVIDE (_alt_partition_RAM_end = ABSOLUTE(.));
    } > RAM

    PROVIDE (_alt_partition_RAM_load_addr = LOADADDR(.RAM));

    .ext_flash :
    {
        PROVIDE (_alt_partition_ext_flash_start = ABSOLUTE(.));
        *(.ext_flash. ext_flash.*)
        . = ALIGN(4);
        PROVIDE (_alt_partition_ext_flash_end = ABSOLUTE(.));
    } > ext_flash

    PROVIDE (_alt_partition_ext_flash_load_addr = LOADADDR(.ext_flash));

    .DDR2 :
    {
        PROVIDE (_alt_partition_DDR2_start = ABSOLUTE(.));
        *(.DDR2. DDR2.*)
        . = ALIGN(4);
        PROVIDE (_alt_partition_DDR2_end = ABSOLUTE(.));
        _end = ABSOLUTE(.);
        end = ABSOLUTE(.);
        __alt_stack_base = ABSOLUTE(.);
    } > DDR2

    PROVIDE (_alt_partition_DDR2_load_addr = LOADADDR(.DDR2));

    /*
     * Stabs debugging sections.
     *
     */

    .stab          0 : { *(.stab) }
    .stabstr       0 : { *(.stabstr) }
    .stab.excl     0 : { *(.stab.excl) }
    .stab.exclstr  0 : { *(.stab.exclstr) }
    .stab.index    0 : { *(.stab.index) }
    .stab.indexstr 0 : { *(.stab.indexstr) }
    .comment       0 : { *(.comment) }
    /* DWARF debug sections.
       Symbols in the DWARF debugging sections are relative to the beginning
       of the section so we begin them at 0.  */
    /* DWARF 1 */
    .debug          0 : { *(.debug) }
    .line           0 : { *(.line) }
    /* GNU DWARF 1 extensions */
    .debug_srcinfo  0 : { *(.debug_srcinfo) }
    .debug_sfnames  0 : { *(.debug_sfnames) }
    /* DWARF 1.1 and DWARF 2 */
    .debug_aranges  0 : { *(.debug_aranges) }
    .debug_pubnames 0 : { *(.debug_pubnames) }
    /* DWARF 2 */
    .debug_info     0 : { *(.debug_info .gnu.linkonce.wi.*) }
    .debug_abbrev   0 : { *(.debug_abbrev) }
    .debug_line     0 : { *(.debug_line) }
    .debug_frame    0 : { *(.debug_frame) }
    .debug_str      0 : { *(.debug_str) }
    .debug_loc      0 : { *(.debug_loc) }
    .debug_macinfo  0 : { *(.debug_macinfo) }
    /* SGI/MIPS DWARF 2 extensions */
    .debug_weaknames 0 : { *(.debug_weaknames) }
    .debug_funcnames 0 : { *(.debug_funcnames) }
    .debug_typenames 0 : { *(.debug_typenames) }
    .debug_varnames  0 : { *(.debug_varnames) }

    /* Altera debug extensions */
    .debug_alt_sim_info 0 : { *(.debug_alt_sim_info) }
}

/* provide a pointer for the stack */

/*
 * Don't override this, override the __alt_stack_* symbols instead.
 */
__alt_data_end = 0xc000000;

/*
 * The next two symbols define the location of the default stack.  You can
 * override them to move the stack to a different memory.
 */
PROVIDE( __alt_stack_pointer = __alt_data_end );
PROVIDE( __alt_stack_limit   = __alt_stack_base );

/*
 * This symbol controls where the start of the heap is.  If the stack is
 * contiguous with the heap then the stack will contract as memory is
 * allocated to the heap.
 * Override this symbol to put the heap in a different memory.
 */
PROVIDE( __alt_heap_start    = end );
PROVIDE( __alt_heap_limit    = 0xc000000 );
